For 1990-2009 cars

### Removal Procedure

1. Depress the center pins inward to release the radio/HVAC controller cover push pin fasteners.

Important: Do not push the center pins through the fasteners.

2. Remove the fasteners and pull the radio/HVAC controller cover rearward.
3. Disconnect the traction control/fog lamp/rear defog electrical connector, if equipped.
4. Remove the radio screws.
5. Push the spring clips in through D holes on both sides of the radio brace.
6. Pull the radio out slightly to access the rear of the radio.
7. Disconnect the electrical connector and antenna.
8. Remove the radio.

### Installation Procedure

1. Connect the electrical connector and antenna to the back side of the radio.
2. Install the radio.

Important: Make sure the spring clips are seated in D holes on both sides.

3. Install and tighten the screws.

Tighten
Tighten the screws to 2.5 N·m (22 lb in) .

4. Connect the traction control/fog lamp/rear defog electrical connector, if equipped.
5. Install the radio/HVAC control cover. Push in at clip locations.
6. Install the push pins and lock.