For 1990-2009 cars

## Head Restraint Replacement SL2/SC2/SW2

### Removal Procedure

1. Raise the headrest assembly to the full up position.
2. Push the headrest lever toward the rear of the vehicle.
3. Pull the headrest out of the seatback.

### Installation Procedure

1. Align the headrest support rods with the holes in the headrest bushing.
2. Push the headrest lever toward the rear of the vehicle.
3. Push the headrest into the seatback.