For 1990-2009 cars

## Automatic Recirculation Switch Replacement Switch

### Removal Procedure

1. Carefully remove the A/C-Recirc switch package by lifting at the outer edge with a small screwdriver.
2. Disconnect the electrical connector.

### Installation Procedure

1. Connect the electrical connector.
2. Install the A/C-Recirc switch package through the opening and push it straight in.

## Automatic Recirculation Switch Replacement Bulb

### Removal Procedure

1. Remove the A/C-Recirc switch package by lifting at the outer edge with a small screwdriver.
2. Turn the bulb socket counterclockwise and remove.

### Installation Procedure

1. Insert the bulb into the opening and turn the clockwise to lock.
2. Install the A/C-Recirc switch package through the opening and push straight in.