For 1990-2009 cars

### DTC Parameters

DTC P0749 is set when there has been a ground/open or short to voltage fault in the pressure control solenoid circuit for a time less than the time required to set DTCs P0768 and P0747, twice per ignition cycle.

### Test Description

This DTC indicates an intermittent condition. Refer to DTC P0746, DTC P0747 and DTC P0748 for circuits that may have intermittent faults. Also refer to Diagnostic Aids for these DTCs.

### Repair Verification

Monitor the DTC menu Code Status for Pass Since Code Clear and Pass This Ignition Cycle. When both have passed, the repair is verified.

Criteria for pass:

• | The engine is running.

• | Power is present at the solenoids and no active faults exist for this solenoid.