For 1990-2009 cars

### Removal Procedure

Caution: If energy absorber is removed or damaged it must be replaced with a new part. If omitted, the vehicle will not meet federal motor vehicle safety standards (FMVSS), subjecting the retailer to possible civil penalties for making the vehicle inoperative to the FMVSS, and increasing the risk of injury to the vehicle occupants.

1. Remove the lower trim panel. Refer to Rear Side Door Trim Panel Replacement .
2. Partially remove the water deflector.
3. Fold in the sides of the lower latch sound barrier and remove.

### Installation Procedure

1. Fold in the sides of the lower latch sound barrier and install into the lower latch cavity. Be sure that the barrier seats into the latch area and the lower latch cable is fitted into the barrier slot.
2. Install the water deflector. Refer to Rear Side Door Water Deflector Replacement . Be sure that there are no wrinkles in the area indicated on the illustration.
3. Install the lower trim panel. Refer to Rear Side Door Trim Panel Replacement .