For 1990-2009 cars

### Removal Procedure

1. Remove inner trim panel. Refer to Rear Side Door Trim Panel Replacement .
2. Grasp inner seal and carefully pull from inner belt flange. Use of a putty knife covered with tape may be needed to gently pry seal from flange.

### Installation Procedure

1. Position seal strip to inner belt flange.
2. Starting at rear, press inner seal into inner belt flange.
3. Install inner trim panel. Refer to Rear Side Door Trim Panel Replacement .