For 1990-2009 cars

Application | Specifications
--- | ---
Metric | English
ABS Bracket-to-Midrail Bolt | 16 N·m | 9 lb ft
Air Box Attachment Bolts | 10 N·m | 89 lb in
Air Cleaner Tube-to-Throttle Body Clamp | 2 N·m | 18 lb in
Battery Case Bracket Stud & Nut | 9 N·m | 80 lb in
Battery Terminal Bolts | 17 N·m | 13 lb ft
Battery Tray-to-Frame Rail Bolts | 10 N·m | 89 lb in
Brake Line Bracket-to-Transaxle Bolt | 5 N·m | 44 lb in
Brake Master Cylinder-to-Booster Nuts | 27 N·m | 20 lb ft
Case-to-Converter Housing (Long Bolts) | 28 N·m | 21 lb ft
Case-to-Converter Housing (Short Bolts) | 25 N·m | 18 lb ft
Case-to-End Cover Dowel Pins | 20 N·m | 15 lb ft
Clamp Support-to-Engine Stiffening Bracket | 31 N·m | 23 lb ft
Clamp Support-to-Front Exhaust Pipe | 60 N·m | 44 lb ft
Console Fasteners | 2.2 N·m | 19 lb in
Control Base Assembly Nuts | 25 N·m | 19 lb ft
End Cover-to-Case Bolts | 28 N·m | 21 lb ft
Engine Strut Bracket-to-Frame Fastener | 50 N·m | 37 lb ft
Engine-to-Transaxle Stiffening Brace Bolts | 54 N·m | 40 lb ft
Exhaust Pipe (Front)-to-Manifold Nuts | 31 N·m | 23 lb ft
Flywheel Housing Cover-to-Converter Housing Bolts | 11 N·m | 8 lb ft
Forward/Reverse Servo Piston Cover-to-Case Bolts | 20 N·m | 15 lb ft
Forward/Reverse Shift Fork-to-Forward/Reverse Servo Piston Bolt | 10 N·m | 89 lb in
Frame-to-Body Bolts | 210 N·m | 155 lb ft
Front Exhaust Pipe-to-Catalytic Converter Nuts | 25 N·m | 18 lb ft
Ground Terminal-to-Converter Housing Nuts | 25 N·m | 19 lb ft
Ignition Module-to-Converter Housing Bolts | 8 N·m | 71 lb in
Input Shaft Clamp Nut | 150 N·m | 111 lb ft
Input Shaft Pilot Hub-to-End Cover Bolts | 12 N·m | 9 lb ft
Input Shaft Pilot Hub-to-End Cover Torx® Bolts | 5 N·m | 44 lb ft
Input Speed Sensor (ISS) | 26 N·m | 19 lb ft
Intake Manifold Support Bracket-to-Intake Manifold Bolt | 30 N·m | 22 lb ft
Intake Manifold Support Bracket-to-Intermediate Shaft Support Bolt | 54 N·m | 40 lb ft
Intermediate Shaft Support Bracket-to-Engine Bolts | 54 N·m | 40 lb ft
Lower Ball Joint-to-Steering Knuckle Nut | 75 N·m | 55 lb ft
Lower Fascia Brace-to-Frame J-nut | 10 N·m | 89 lb in
Lower Mount-to-Frame Nut | 48 N·m | 35 lb ft
Lower Mount-to-Transaxle Bolts | 32 N·m | 24 lb ft
Manual Detent Lever-to-Manual Detent Shaft Nut | 12 N·m | 9 lb ft
Output Shaft Clamp Nut | 150 N·m | 111 lb ft
Output Speed Sensor (OSS) | 26 N·m | 19 lb ft
PCM J1 Connector-to-PCM Bolt | 8 N·m | 71 lb in
PCM-to-Battery Tray Bolts | 6 N·m | 53 lb in
Park Pawl Assembly-to-Converter Housing Bolts | 30 N·m | 22 lb ft
Pump-to-Converter Housing Bolts | 12 N·m | 9 lb ft
Shifter Cable Pass-Through Grommet Nuts | 7 N·m | 62 lb in
Stator Shaft-to-Pump Bolts | 30 N·m | 22 lb ft
Steering Gear-to-Frame Fasteners | 50 N·m | 37 lb ft
Stop Lamp Switch Mounting Nut | 10 N·m | 89 lb in
Torque Converter-to-Flexplate Bolts | 70 N·m | 52 lb ft
Transaxle Bracket-to-Case Bolts | 54 N·m | 40 lb ft
Transaxle Control Lever-to-Manual Detent Shaft Nut | 12 N·m | 9 lb ft
Transaxle Cooler Line Fitting-to-Case | 25 N·m | 18 lb ft
Transaxle Cooler Line Fitting-to-Radiator | 14 N·m | 10 lb ft
Transaxle Drain Plug | 30 N·m | 22 lb ft
Transaxle Electrical Connector Bolt | 3 N·m | 27 lb in
Transaxle Filter Tube | 31 N·m | 23 lb ft
Transaxle Fluid Temperature Sensor-to-Case | 8 N·m | 71 lb in
Transaxle Oil Indicator Tube-to-Case Bolt | 12 N·m | 9 lb ft
Transaxle Range Switch-to-Case Bolts | 14 N·m | 10 lb ft
Transaxle Solenoid Harness Connector Bolt | 2.5 N·m | 22 lb ft
Transaxle Strut Frame Bracket-to-Frame Nut | 50 N·m | 37 lb ft
Transaxle Strut-to-Midrail Bolt | 70 N·m | 52 lb ft
Transaxle Strut-to-Midrail Bracket Bolt | 70 N·m | 52 lb ft
Transaxle Strut-to-Transaxle Bracket Bolt | 70 N·m | 52 lb ft
Transaxle-to-Engine Bolts | 130 N·m | 96 lb ft
Transaxle-to-Engine Studs | 100 N·m | 74 lb ft
Valvebody Assembly Bolts | 11 N·m | 8 lb ft
Valvebody Cover-to-Case Bolts | 12 N·m | 9 lb ft
Wheel Lug Nuts | 140 N·m | 103 lb ft