For 1990-2009 cars

### Removal Procedure

Important: LHD shown, RHD similar.

1. Remove the front seats. Refer to Front Seat Replacement - Bucket in Seats.
2. Remove the console. Refer to Console Replacement in Instrument Panel, Gages, and Console.
3. Remove the front lower garnish molding by firmly pulling at the clip locations.
4. Remove the rear cushion. Refer to Rear Seat Cushion Cover Replacement in Seats.
5. On coupe, remove the quarter lower trim finish panel. Refer to Rear Quarter Trim Panel Replacement - Right Side .
6. Remove the rear carpet retainer by firmly pulling at the clip location.
7. Remove the center pillar lower molding by firmly pulling at the clip locations.
8. Remove the carpet by guiding it off of the fuel door/rear compartment release levers.
9. Remove the carpet from the vehicle.

### Installation Procedure

Important: LHD shown, RHD similar.

1. Install the carpet into the vehicle.
2. Guide the carpet around the fuel door/rear compartment release levers.
3. Tuck under and around the instrument panel center location. Install the center pillar lower molding by firmly pushing at the clip locations.
4. Install the front lower garnish molding by firmly pushing at the clip locations.

Important: On the coupe, be certain to observe the orientation and torque requirements of the slide bar because it is crucial to correct the operation of the seat belt system.

5. Install the rear carpet retainer by firmly pushing at the clip locations.
6. On the coupe, install the quarter lower trim finish panel. Refer to Rear Quarter Trim Panel Replacement - Right Side .
7. Install the rear seat cushion. Refer to Rear Seat Cushion Cover Replacement in Seats.
8. Install the center console. Refer to Console Replacement in Instrument Panel, Gages, and Console.
9. Install the front seats. Refer to Front Seat Replacement - Bucket in Seats.