For 1990-2009 cars

### Removal Procedure

1. Remove the air induction system. (DOHC shown, SOHC similar.)
2. Disconnect the negative battery cable from the battery.
3. Disconnect the positive battery cable from the battery.
4. Remove the hold-down retaining nut (1) and screws (2), and lift off the battery hold-down retainer (3).
5. Lift the battery out of the vehicle, and place it in a safe location.

Important: One bolt is located in the fender wall.

6. Remove the battery tray.
7. Disconnect the back-up light electrical connector.
8. Place the transaxle in neutral.
9. Remove the shift control housing retaining bolts.
10. Remove the housing and the gasket.

### Installation Procedure

1. Clean the gasket surfaces and install the shift housing gasket to the case.

Notice: Make sure the shift housing is completely down on case before installing bolts. Torquing bolts on a misaligned housing will damage the case.

Important: Clean and lubricate the fastener with Saturn Transaxle Fluid. Wipe off the excess fluid and install.

2. Install the shifter housing assembly on the case.

Tighten
Tighten the shift control housing-to-case bolts to 28 N·m (21 lb ft).

3. Connect the back-up light switch electrical connector.
4. Install the battery tray.
5. Torque the battery tray bolts.

Tighten
Tighten the battery tray bolts to 10 N·m (89 lb in).

6. Make sure the battery tray is clean.
7. Make sure that the battery cable ends are clean and free of corrosion. (Clean with a wire brush.)
8. Make sure that the battery is in good physical condition (e.g., no cracks, or obvious damage) and that the terminals are clean.
9. Install the battery carefully in the battery tray; make sure that the terminals do not short against any metal during the installation.
10. Install the battery hold-down retainer (3), locking the battery into the tray. Install and tighten the hold-down retainer nut (1) and screws (2).

Tighten
Tighten the battery hold down-to-battery tray fasteners to 9 N·m (80 lb in).

11. Install the positive battery cable first.

Tighten
Tighten the battery terminal bolts to 17 N·m (151 lb in).

12. Install the negative battery cable last.

Tighten
Tighten the battery terminal bolts to 17 N·m (151 lb in).

13. Install the air induction system. (DOHC shown, SOHC similar.)