For 1990-2009 cars

### Left Front Motor Circuit Shorted To B+

If a motor circuit is shorted to battery, ABS will be disabled and the antilock telltale lamp will be turned On.

### Code Parameters

Code 58 sets if:

LF motor circuit is shorted to B+

This code can set at all times except when a previous failure has disabled ABS operation.

### Diagnostic Aids

When attempting to diagnose an intermittent problem, use the Scan tool to review supplemental diagnostic information. The supplemental data can be used to duplicate a problem.

Select Malf History from scan tool ABS menu.

Check the tightness of the female terminal grip with a spare male terminal.