For 1990-2009 cars

### Removal Procedure

Notice: Rotating the screwdriver while removing the switch may damage the steering wheel.

1. Use a small flat-blade screwdriver to pry the switch assembly from the steering wheel.
2. Disconnect the cruise switch harness connector.

### Installation Procedure

1. Connect the cruise switch harness connector. Push in the connector until a click is felt and pull back to confirm engagement.
2. Insert the cruise switch assembly in the steering wheel and gently apply pressure to fasten the switch in the opening.