For 1990-2009 cars

If the transaxle fluid is milky pink in color, it is possible that there has been a transaxle oil cooler leak and the transaxle fluid is contaminated with engine coolant. If this condition exists, drain and fill the transaxle fluid and the engine coolant and replace the following components:

• | The radiator

• | The cooler lines

• | The torque converter

• | The valve body and solenoids

• | The clutch pistons

• | The clutch plates

• | The suction filter

• | The pressure filter

• | Gasket, seals, O-rings (automatic transaxle gasket/seal kit)