For 1990-2009 cars

### Circuit Description

The powertrain control module (PCM) provides approximately 12 volts ignition voltage to control the movement of the cruise module motor. The feedback signal is internal to the PCM monitors circuit 1886 and compares low vs. high as the QDM driver is turned ON and OFF. If voltage is too high when the QDM driver is OFF, DTC P1581 will set.

### Conditions for Setting the DTC

Important: The cruise move circuit is tested continuously anytime the ignition is ON.

DTC P1581 will set if circuit 1886 is greater than 3 volts with the QDM driver OFF.

### Diagnostic Aids

If an intermittent exists, observe the scan tool parameters while moving connectors and harnesses.