For 1990-2009 cars

### Removal Procedure

1. Remove the front fascia. Refer to Front Bumper Fascia Replacement .
2. Remove the fascia support-to-bumper impact bar attaching nuts.
3. Slide the fascia support off of the studs.

### Installation Procedure

1. Position the fascia support to the impact bar.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the nuts to the studs attaching the fascia support to the bumper impact bar.

Tighten
Tighten the nuts to 3.5 N·m (31 lb in)

3. Install the front fascia. Refer to Front Bumper Fascia Replacement .