For 1990-2009 cars

## Window Guide Channel Replacement - Front Door Coupe

### Removal Procedure

1. Remove the front door window. Refer to Front Side Door Window Replacement . The outer door panel is removed in the illustration to show the location.
2. Remove the front door window upper weatherstrip from the guide. Refer to Window Guide Channel Replacement - Front Door .
3. Remove the attaching fasteners and remove the rear window guide.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the rear window guide with 2 rivets and 1 nut.

Tighten
Tighten the front door rear window guide bolt to 6 N·m (53 lb in).

2. Install the front door window upper weatherstrip. Refer to Window Guide Channel Replacement - Front Door .
3. Install the front door window. Refer to Front Side Door Window Replacement .
4. Check the window for proper operation.
5. Install the door trim panel. Refer to Front Side Door Trim Panel Replacement .

## Window Guide Channel Replacement - Front Door Sedan/Wagon

### Removal Procedure

1. Remove the front door window. Refer to Front Side Door Window Replacement . The outer door panel is removed in the illustration to show the location.
2. Remove the front door rear applique. Refer to Rear Door Frame Applique Replacement .
3. Remove the front door window upper weatherstrip from the guide. Refer to Window Guide Channel Replacement - Front Door .
4. Partially remove the inner sealing strip (belt seal).
5. Partially remove the front door window secondary weatherstrip.
6. Remove the 2 rivets and 1 nut and remove the window guide.

### Installation Procedure

1. Install the window guide with the 2 rivets using the Marson HP2 riveter, or equivalent. Press the riveter tip into the channel flush with the surface.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the nut to the guide.

Tighten
Tighten the front door rear window guide bolt to 6 N·m (53 lb in).

3. Install the front door window secondary weatherstrip. Refer to Front Side Door Upper Auxiliary Weatherstrip Replacement .
4. Install the inner sealing strip (belt seal).
5. Install the front door window upper weatherstrip. Refer to Window Guide Channel Replacement - Front Door .
6. Install the front door rear applique. Refer to Rear Door Frame Applique Replacement .
7. Install the front door window. Refer to Front Side Door Window Replacement .