For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Brake Pedal Travel | 57.0 mm | 2.25 in
Brake pedal travel maximum with 445 N (100 lbs) force applied to pedal with ignition OFF and vacuum assist depleted. | -- | --

#### Brake Pipes Master Cylinder

Reference Number | Circuit | Nut Sizer Base | Torque | ABS
--- | --- | --- | --- | ---
1* | LF | M1 x 1.0 | -- | 31 N·m (24 lb ft)
2 | RR | M10 x 1.0 | --
3 | LR | M13 x 1.5 | --
4 | RF | M11 x 1.5 | --
Front* | LF/RF | -- | M12 x 1.0
Rear* | LR/RR | M11 x 1.5
*Brake pipe is available to service as complete assembly.

#### Brake Pipes to Brake Hose

Reference Number | Circuit | Nut Size | Torque
--- | --- | --- | ---
*1 | LF | M12 x 1.0 | 19 Nm (11 lb ft)
2 | RR | M10 x 1.0
3 | LR
4 | RF
*Brake pipe is available to service as complete assembly

#### Brake Pipes to ABS Assembly

Reference Number | Circuit | Nut Size | Torque
--- | --- | --- | ---
*1 | LF | M10 x 1.0 | 32 Nm (24 lb ft)
2 | RR | M11 x 1.5
3 | LR | M10 x 1.0
4 | RF | M11 x 1.5
*5 | Front | M11 x 1.5
*6 | Rear | M11 x 1.5
*Brake pipe is available to service as complete assembly

#### Brake Pipes to Union

Union Size | Nut Size | Torque
--- | --- | ---
M10 x 1.0 Female Connector | M10 x 1.0 | 15 Nm (11 lb ft)