For 1990-2009 cars

### Circuit Description

When torque converter clutch (TCC) is commanded OFF, the engine speed to input shaft speed ratio (delta) is monitored to assure TCC is OFF. TCC stuck ON indicates that TCC was commanded OFF but the actual ratio (delta) across the torque converter, engine speed/turbine shaft speed, is 1 to 1 or TCC is ON. TCC is turned OFF by opening circuit 422 at the PCM/TC. A TCC stuck ON will usually cause the engine to stall when reverse is selected.

### Conditions for Setting the DTC

DTC P0742 is set when the PCM has detected the following conditions for more than 4 seconds twice per ignition cycle:

• | Engine speed is greater than 908 RPM.

• | Input shaft speed is between 224-2,800 RPM.

• | TCC is commanded to release for more than 0.25 seconds.

• | Load value, engine torque, is greater than 100.

• | Speed delta, engine speed -- turbine shaft speed, across torque converter is less than 84 RPM.

### Test Description

Numbered steps below refer to numbered steps on the chart.

1. Check for DTCs P0740 and P0744. They must be eliminated first as a possible cause of DTC P0742.

Important: To check solenoid operation, command the solenoid quick test using the scan tool.

2. Check the solenoid operation. Use the solenoid quick check in the test section located at the end of the DTC charts. The solenoid quick test will PWM the solenoids at a set rate. Listen and compare the noise of the TCC gear actuator to that of other solenoids. The noise of all should be similar.
3. The TCC release circuit may be leaking at the seal ring on the input shaft. This would allow release pressure to leak off to the converter out circuit or lube circuit. Also a remote possibility is the ball pressed into the input shaft is loose.

### Repair Verification

Monitor the DTC menu Code Status for Pass Since Code Clear and Pass This Ignition Cycle. When both have passed, the repair is verified.

Criteria for pass:

• | The TCC is commanded OFF.

• | The speed ratio across the torque converter is less than 1:1 for 12 seconds.

### Diagnostic Aids

• | When the PCM detects a fault in the circuit, an open, ground or short, the PCM will open the circuit internally to protect the circuit.

• | The TCC may be detected as stuck on when the transaxle is put into drive range. If TCC is stuck on at start-up, a stall may occur, and after a restart it will result in a 3rd or 4th gear start.