For 1990-2009 cars

### Removal Procedure

1. Remove the headlamp housing. Refer to Headlamp Assembly or Headlamp Bulb Replacement in Lighting Systems.
2. Remove the nuts attaching the fog lamp bracket to the impact bar.
3. Remove the fog lamp assembly down through the bottom of the front fascia.
4. Remove fog lamp assembly from fog lamp bracket.

### Installation Procedure

1. Install fog lamp assembly to fog lamp bracket.
2. Place the fog lamp assembly into position through the bottom of the front fascia.

Notice: Refer to Fastener Notice in the Preface section.

3. Install the nuts attaching the fog lamp bracket to the impact bar.

Tighten
Tighten the fog lamp bracket-to-impact bar attaching nuts to 30 N·m(22 lb ft).

4. Install the headlamp housing. Refer to Headlamp Assembly or Headlamp Bulb Replacement in Lighting Systems.
5. Aim the fog lamp. Refer to Fog Lamp Aiming in Lighting Systems.