For 1990-2009 cars

## Instrument Cluster Replacement Left Hand Drive

### Removal Procedure

1. Disable the SIR System.
2. Remove the screws from the DLC connector and steering filler panel.
3. Remove hood release cable from lever.
4. Remove steering column filler panel.
5. Disconnect ignition switch electrical connector at right steering column bolt.
6. Remove steering column bolts and lower column on front seat.
7. Remove fasteners and pull instrument cluster trim bezel rearward at clip locations.
8. Disconnect electrical connector from instrument panel dimmer switch.
9. Remove connector position assurance (CPA) devices and disconnect electrical connectors from instrument panel cluster assembly by squeezing tabs on each side of connector.
10. Remove front and rear instrument panel cluster assembly screws.
11. Remove instrument panel cluster assembly.

### Installation Procedure

1. Install instrument panel cluster assembly.
2. Install and tighten instrument panel cluster assembly screws.
3. Connect electrical connectors to I/P cluster assembly.
4. Install CPA devices.
5. Connect electrical connector to I/P dimmer switch.
6. Install instrument cluster trim bezel. Push in at clip locations.
7. Install push pin fasteners.
8. Raise steering column into position.
9. Install and torque bolts.

Tighten
Tighten bolts to 35 N·m (26 lb ft)

10. Connect ignition switch electrical connector at right steering column bolt.
11. Install hood release cable to lever.
12. Install steering column filler panel and DLC connector.
13. Install and tighten screws.
14. Enable the SIR System.

## Instrument Cluster Replacement Right Hand Drive Domestic

### Removal Procedure

1. Disable the SIR System. Refer to Disabling the SIR System.
2. Remove the screws from the data link connector (DLC) and the steering column filler panel.
3. Lower the steering column filler panel and remove the hood release handle assembly.
4. Disconnect the ignition switch electrical connector at the right steering column bolt.
5. Remove the steering column bolts and the lower column onto the front seat.
6. Remove the fasteners and pull the instrument cluster trim bezel rearward at the clip locations.
7. Disconnect the electrical connector from the instrument panel dimmer switch and the defroster switch.
8. Remove the connector position assurance (CPA) devices and disconnect the electrical connectors from the instrument cluster by squeezing the tabs on each side of the connector.
9. Remove the front and the rear instrument cluster screws.
10. Remove the instrument cluster.

### Installation Procedure

1. Install the instrument cluster.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the front and the rear screws.

Tighten
Tighten the rear screws to 3 N·m (26 lb in).

3. Connect the electrical connectors to the instrument cluster.
4. Install the CPA.
5. Connect the electrical connector to the dimmer switch and defroster switch.
6. Install the instrument cluster trim bezel. Push in at the clip locations.
7. Install the push pin fasteners.
8. Raise the steering column into position.
9. Install and torque the bolts

Tighten
Tighten the bolts to 35 N·m (26 lb ft).

10. Connect the ignition switch electrical connector at the right steering column bolt.
11. Install the hood release handle assembly to the steering column filler panel.

Tighten
Tighten the handle to 1.5 N·m (13 lb in).

12. Install the steering column filler panel and the DLC.
13. Install and torque the screws.

Tighten
Tighten the screws to 2.2 N·m (20 lb in).

14. Enable the SIR System. Refer to Enabling the SIR System.