For 1990-2009 cars

## Seat Back Beam Latch Replacement - Rear Wagon

### Removal Procedure

1. Remove the rear seat back beam latch assembly. Refer to Seat Back Beam Latch Replacement - Rear .
2. Remove the bolts attaching the latch to the rear seat back beam assembly and remove the latch.

### Installation Procedure

1. Apply Loctite 242® Threadlocker P/N 21485277, or equivalent, to the latch bolts.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the rear seat back beam latch to the rear seat back beam assembly and secure with the latch bolts.

Tighten
Tighten the rear folding seat back latch fasteners to 2 N·m (18 lb in).

3. Install the rear seat back beam latch assembly. Refer to Seat Back Beam Latch Replacement - Rear .