For 1990-2009 cars

### Removal Procedure

1. Raise the hood to the open position. Support the hood with a prop rod.
2. Remove the retainer clips by inserting a trim tool between the clip head and the insulator and prying the clips out.
3. Remove the hood insulator.

### Installation Procedure

1. Position the front of the insulator under the retainer tabs located at the front center of the hood inner panel.
2. Install two center clips to hold the insulator in position by positioning clip through insulator and pushing into holes in the hood inner panel.
3. Align the insulator as necessary. Install the remainder of the clips.
4. Lower the prop rod and close the hood.