For 1990-2009 cars

### Removal Procedure

Important: Energy absorber must be replaced if it is damaged, cracked, broken or crushed.

1. Remove the top cover.
2. Scrape all the material from the cross car beam using a putty knife or gasket scraper.

Important: Make sure solvent does not contact plastic I/P parts.

3. Clean all adhesive from the cross car beam with solvent.

### Installation Procedure

1. Peel off the backing from the energy absorber.
2. Install the energy absorber to the cross car beam in the original position.
3. Install the top cover.