For 1990-2009 cars

## Front Side Door Window Belt Outer Sealing Strip Replacement Sedan/Wagon

### Removal Procedure

1. Remove retaining screw from sealing strip end cap.
2. Remove mirror trim panel and remove foam filler, then loosen mirror.
3. Carefully lift up on outer sealing strip starting at rear and working forward.

### Installation Procedure

1. Install by sliding forward end of sealing strip beneath mirror.
2. Align rear sealing strip end cap retainer with hole for end cap retaining screw.
3. Starting at rear of seal strip push sealing strip down onto flange until fully seated.

Notice: Refer to Fastener Notice in the Preface section.

4. Tighten mirror attaching nuts.

Tighten
Tighten the outside rear view mirror nuts to 10 N·m (89 lb in).

5. Install foam filler and mirror trim panel.
6. Tighten sealing strip retaining screw.

Tighten
Tighten the outer sealing strip - belt seal (Sedan/Wagon) to 6 N·m (53 lb in).

## Front Side Door Window Belt Outer Sealing Strip Replacement Coupe

### Removal Procedure

1. Remove fastener from sealing strip end cap.
2. Remove mirror trim panel and remove foam filler and loosen mirror.
3. Carefully lift up on outer sealing strip starting at rear and working forward.

### Installation Procedure

1. Install by sliding forward end of sealing strip beneath mirror.
2. Align rear sealing strip end cap retainer with hole for end cap retaining screw.
3. Starting at rear of sealing strip, push sealing strip down onto flange until fully seated.

Notice: Refer to Fastener Notice in the Preface section.

4. Tighten mirror attaching nuts.

Tighten
Tighten the outside rear view mirror nuts to 10 N·m (89 lb in).

5. Install foam filler and mirror trim panel.
6. Install sealing strip fastener.