For 1990-2009 cars

## Inflatable Restraint Side Impact Sensor Replacement Coupe

### Removal Procedure

Notice: Do not use sensor if dropped from any height.

1. Disable the SIR system. Refer to Disabling the SIR System .
2. Remove inside door trim panel. Refer to Front Side Door Trim Panel Replacement in Doors.
3. Peel back the water deflector.
4. Disconnect the SIS connector.
5. Loosen the SIS fasteners.
6. Slide the sensor assembly out of the slotted holes.
7. Remove the SIS.

### Installation Procedure

1. Loosen the fasteners on the SIS assembly.
2. Position the SIS in the slotted holes in the door structure (bolt head facing inboard).

Notice: Refer to Fastener Notice in the Preface section.

3. Secure the fasteners.

Tighten
Tighten the SIS Fasteners to 10 N·m (89 lb in).

4. Connect the SIS connector and insert the connector position assurance (CPA) to secure.
5. Reposition the water deflector.
6. Install the inside door trim panel. Refer to Front Side Door Trim Panel Replacement in Doors.
7. Enable the SIR system. Refer to Enabling the SIR System .