For 1990-2009 cars

## Cruise Control Module Rod Adjustment Left Hand Drive

1. Remove the air intake tube at the throttle body.
2. Observe the position of the throttle plate.

Important: 1-2 mm (0.04-0.079 in) is approximately 1 click movement of the adjuster.

3. Depress the release tab on the adjuster and slide the adjuster away from the bracket. Move the adjuster toward the bracket to gain 1-2 mm (0.04-0.079 in) clearance between the adjuster and the accelerator pedal bracket. If using the PDT, scan tool, verify the closed throttle position (TP) voltage prior to adjustment. Ensure after adjustment that the throttle position voltage is unchanged.

Notice: Driveability concerns may result if the cruise control rod is not adjusted properly.

4. Install the air intake tube.

## Cruise Control Module Rod Adjustment Right Hand Drive Domestic

1. Cruise cable adjuster
2. Cruise cable module
3. Cruise control rod adjustment: 1-2 mm clearance between the adjuster and accelerator pedal.

1. Remove the air intake tube at the throttle body.
2. Observe the position of the throttle plate.

Important: 1-2 mm (0.04-0.079 in) is approximately 1 click movement of the adjuster.

3. Depress the release tab on the adjuster and slide the adjuster away from the bracket. Move the adjuster toward the bracket to gain 1-2 mm (0.04-0.079 in) clearance between the adjuster and the accelerator pedal bracket. If using the PDT, scan tool, verify the closed throttle position (TP) voltage prior to adjustment. Ensure after adjustment that the throttle position voltage is unchanged.

Notice: Driveability concerns may result if the cruise control rod is not adjusted properly.

4. Install the air intake tube.