For 1990-2009 cars

Important: When performing a wheel alignment after any suspension system component removal and installation, the vehicle must be driven and/or the suspension system worked, manually bounced at least 20 times, to allow the components to locate properly before the alignment adjustment.

First: Rear Camber
Second: Rear Toe
Third: Right Front Camber and Caster
Fourth: Left Front Camber and Caster
Fifth: Front Toe