For 1990-2009 cars

Notice: Refer to Fastener Notice in the Preface section.

1. For window fore aft adjustment, lower the window to the 3/4 down position. Push rearward to seat in the rear window guide. Bring pressure against the rear window guide and tighten the guide bolt.

Tighten
Tighten the rear window regulator bolts to 10 N·m (89 lb in).

2. Check for proper operation.
3. Adjust the window regulator rear bolt, as required.

Tighten
Tighten the rear window regulator bolts to 10 N·m (89 lb in).