For 1990-2009 cars

## Quarter Window Garnish Molding Replacement Coupe Left Side 1st Design

### Removal Procedure

1. Remove the seat belt retractor cover by pulling.
2. Remove the coat hook. Refer to Coat Hook Replacement .
3. Remove the quarter window garnish upper molding by pulling. Refer to the following:

• | Quarter window garnish upper molding (1)

• | Interlock tab (2)

### Installation Procedure

1. Install the quarter window garnish upper molding. Refer to the following:

• | Quarter window garnish upper molding (1)

• | Interlock tab (2)

2. Install the seat belt retractor cover panel.
3. Install the coathook. Refer to Coat Hook Replacement .