For 1990-2009 cars

### Removal Procedure

1. Open the armrest cover
2. Remove the armrest fasteners and the left armrest out of the center console.

### Installation

1. Install the armrest assembly into the console rear storage tray, open the armrest cover and install the screws.

Notice: Refer to Fastener Notice in the Preface section.

2. Tighten the screws.

Tighten
Tighten the screws to 1.6 N·m (14 lb in).