For 1990-2009 cars

### Removal Procedure

1. Disconnect the air pump harness connector.
2. Remove the air pump wiring harness from the bracket.
3. Remove the outlet air hose.
4. Remove the mounting bolt.
5. Remove the air pump from the air pump bracket.

### Installation Procedure

1. Install the air pump into the air pump bracket.

Notice: Refer to Fastener Notice in the Preface section.

2. Install and torque the bolt.

Tighten
Tighten the air pump-to-air pump bracket 5.5 N·m (49 lb in).

3. Install the outlet air hose to the air pump air outlet port.
4. Connect the air pump harness connector. Push in the connector until a click is heard and pull back to confirm a positive engagement.
5. Install the air pump wiring harness on the bracket.