For 1990-2009 cars

## Steering Column Opening Filler Replacement LHD

### Removal Procedure

1. Remove the steering column filler panel fasteners.
2. Remove the hood release cable from the lever by releasing the cable housing, then rotating the cable downward to the cutout.
3. Remove the steering column filler panel.

### Installation Procedure

1. Route the hood release cable through the I/P retainer.
2. Install the hood release cable to the lever.
3. Install the steering column filler panel.

Notice: Refer to Fastener Notice in the Preface section.

4. Install the fasteners.

Tighten
Tighten the steering column filler panel fasteners to 2.2 N·m (19 lb in).

## Steering Column Opening Filler Replacement RHD Domestic

### Removal Procedure

1. Remove the steering column filler panel fasteners.
2. Remove the hood release handle assembly.
3. Remove the steering column filler panel.

### Installation Procedure

1. Install the hood release handle assembly to the steering column filler panel.
2. Install the hood release handle assembly fasteners.

Notice: Refer to Fastener Notice in the Preface section.

3. Install the steering column filler panel.

Tighten
Tighten the steering column filler panel fasteners to 2.2 N·m (19 lb in).