For 1990-2009 cars

Table 1: | Maxifuses
Table 2: | Minifuses Circuit Feeds
Table 3: | Relay Circuit Feeds
Table 4: | Minifuses Circuit Feeds
Table 5: | Relay Circuit Feeds

The wiring circuits in your vehicle are protected from short circuits by fuses. This greatly reduces the chance of circuit overload and fires caused by electrical problems.

There are two fuse blocks called "junction blocks," one is the "underhood junction block," the other is the "instrument panel junction block." To identify and check fuses and relays, refer to the Fuse Usage Chart inside the fuse panel door, near the passenger's left leg for the instrument panel junction block. Remove the fuse panel door to access the fuse and relays.

The underhood junction block is located in the forward part of the engine compartment near the battery. Six spare minifuses and a fuse-puller are located in the underhood junction block. These spare minifuses can be used to replace underhood and instrument panel junction block minifuses.

Replace spare fuses as they are used as soon as you can. To identify and check fuses and relays, refer to the fuse and relay usage chart inside the fuse block cover. To remove a fuse, place the wide end of the fuse puller over the plastic end of the fuse. Squeeze the ends over the fuse and pull the fuse out. A fuse puller is also located on the instrument panel junction block panel access door.

Look at the silver-colored band inside the fuse. If the band is broken or melted, replace the fuse. Be sure you replace a bad fuse with a new one of the same amperage.

### Underhood Fuse Junction Block

This chart lists the maxifuses and the minifuses they control and the following chart lists the systems they control.

#### Maxifuses

NUMBER | FUSE | COLOR (AMP) | MINIFUSE (AMP) OR SYSTEM
--- | --- | --- | ---
1 | PWR CONVCE | Green (30) | Feeds directly to power window relay. SUN (15) (after power window relay).
2 | IGN 3 | Green (30) | IGN 3 (10), Cruise (5)
5 | IGN 4 | Green (30) | IGN 1 (10), TURN (10), B/U LP (10), EGR (10), EIS (10), PCM I (10), INJ (10), WIPER (25), AIR BAG (10), RADIO (IGN) (10)
6 | IP BATT | Green (30) | Body (10), Locks (20), Chime (10), Lighter (20), F Pump (10), TRS 3/4 (10), TRS 2/TCC (10), TRS LP (10), (after fuel pump relay).
7 | COOLING FAN | Green (30) | Feeds directly to engine cooling fan relay
8 | ABS | Green (30) | Feeds directly to ABS enable relay.

### Underhood Fuse Junction Block Minifuses

The following chart lists the minifuses, located in the underhood junction block, and the systems they control.

#### Minifuses Circuit Feeds

FUSE | COLOR (AMP) | SYSTEM
--- | --- | ---
HORN | Red (10) | Horn
R HDLP | Red (10) | Right Headlamps
L HDLP | Red (10) | Left Headlamps
FOG LP | Blue (15) | Fog Lamps
EGR | Red (10) | Linear EGR Solenoid, Evaporative Emmission Canister Purge Solenoid, Heated Oxygen Sensor, Powertrain Control Module
TRS LP | Red (10) | Automatic Transaxle Line Pressure Actuator
A/C | Red (10) | Air Conditioning System
BRAKE | Red (10) | Brake Lamps
PCM I | Red (10) | Powertrain Control Module
EIS | Red (10) | Electronic Ignition System
TRS 3/4 | Red (10) | Automatic Transaxle 3rd Gear Actuator and 4th Gear Actuator
PCM B | Red (10) | Powertrain Control Module Memory
INJ | Red (10) | Fuel Injectors
B/U LP | Red (10) | Backup Lamps, Coolant Level Switch
TRS 2/TCC | Red (10) | Automatic Transaxle 2nd Gear and Torque Converter Clutch Actuator
BRAKE | Red (10) | Brake Lamps
ABS | Red (10) | Anti-Lock Brake System Memory ABS Relay
ABS SOL | Red (10) | ABS Solenoid, ABS Relay
PARK | Red (10) | Front Park Lamps, Taillamps, Front Marker Lamps, Rear Tail Lamps, License Plate Lamps, Radio Display Lights, I/P Cluster Backlighting, I/P Dimmer, Cigar Lighter Ring, Ashtray Light, PRND32 Light, HVAC Control Switch Backlighting
HAZARD | Red (10) | Hazard Flasher, HBTT (Headlamp HI Beam Indicator), I/ P Cluster
RR DFG | Green (30) | Rear Window Defogger
Diode
A/C Diode |  | AC Diode (for Electrical System Protection)

### Underhood Junction Block Relays

The following chart lists the relays, located in the underhood junction block, and the systems they control.

#### Relay Circuit Feeds

RELAY | MAXIMUM LOAD | SYSTEM
--- | --- | ---
A/C | 30 Amp | Air Conditioning System
COOL FAN | 30 Amp | Engine Cooling Fan
FOG LAMP | 30 Amp | Fog Lamps
DRL | 30 Amp | Daytime Running Lamps
ABS | 30 Amp | Anti-lock Brakes (Non-Interchangeable with Other Relays)

### Instrument Panel Junction Block Minifuses

The following chart lists the minifuses, located in the instrument fuse block, and the systems they control.

Note: Fuses are numbered in instrument panel junction block. A label is provided on the fuse block cover for fuse layout.

#### Minifuses Circuit Feeds

NUMBER | FUSE | COLOR (AMP) | SYSTEM
--- | --- | --- | ---
2 | RADIO | Red (10) | Radio
3 | WIPER | Natural (25) | Windshield Wipers and Washers (Front)
4 | IGN 1 | Red (10) | I/P Cluster Telltale & Gages, Chime,Saturn Security System
5 | TURN | Red (10) | Turn Signals, Brake Transaxle Shift Interlock
6 | AIR BAG | Red (10) | Air Bags, Sensing and Diagnostic Module (SDM)
8 | HVAC | Blue (15) | HVAC Controls
9 | IGN 3 | Red (10) | Anti-Lock Brakes, Power Wiindows, Air Conditioning, Traction Switch, Rear Defogger, DRL Relay, Generator
10 | CRUISE | Tan (5) | Cruise Control Switch, Brake Switch
12 | LOCKS | Yellow (20) | Power Door Locks
13 | LIGHTER | Yellow (20) | Cigar Lighter
14 | CHIME | Red (10) | Radio/Clock Memory, Chime Module, Cargo Light (Wagon), Hatch Ajar Indicator Light (Wagon), Saturn Security System
15 | BODY | Red (10) | Dome Lamp, Luggage Compartment Lamp, Outside Remote Mirrors, Map Lights, Wagon Hatch Release, Decklid Release, Power Door Locks
17 | SUN | Blue (15) | Power Sunroof, Rear Wiper/Washer (Wagon)
18 | F PUMP | Red (10) | Electric Fuel Pump

### Instrument Panel Junction Block Relays/Modules

The following chart lists the relays and modules, located in the instrument panel fuse block, and the systems they control.

#### Relay Circuit Feeds

RELAY/MODULE | MAXIMUM LOAD | SYSTEM
--- | --- | ---
POWER WINDOW | 35 AMP | Power Windows, Power Sunroof, Rear Wiper/Washer (Wagon)
F PUMP | 35 AMP | Electric Fuel Pump, Trans. Actuators
RR DEFOG | 35 AMP | Rear Defogger
HVAC BLOWER RELAY | 35 AMP | HVAC Blower Motor
DOOR LOCK RELAY | 20 AMP | Door Lock (Lock)
DOOR LOCK RELAY | 20 AMP | Door Lock (Unlock)
FLASHER MODULE | 6 Bulbs | Turn Signal/Hazard Flashers (Back Side of IPJB)
CHIME MODULE |  | Chime, Rear Defog Timmer (Back Side of IPJB)