For 1990-2009 cars

### Removal Procedure

1. Remove latch cover by inserting a small screwdriver blade at the upper right and lower left corner sections.
2. Apply pressure to force sections outward to disengage clips.
3. Remove four latch assembly fasteners.
4. Remove latch assembly.

### Installation Procedure

1. Position latch assembly on seat back.
2. Install four latch assembly fasteners.
3. Install latch cover by applying pressure at the upper right and lower left corners to engage clips.