For 1990-2009 cars

### Removal Procedure

Caution: Ensure that the vehicle is properly supported and squarely positioned. To help avoid personal injury when a vehicle is on a hoist, provide additional support for the vehicle on the opposite end from which the components are being removed.

1. Position the vehicle on the hoist and ensure the ignition is OFF.

Caution: To avoid any vehicle damage, serious personal injury or death when major components are removed from the vehicle and the vehicle is supported by a hoist, support the vehicle with jack stands at the opposite end from which the components are being removed and strap the vehicle to the hoist.

2. Raise the vehicle.
3. Disconnect the output speed sensor (OSS) harness connector and remove the sensor.

### Installation Procedure

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

Important:

• | Inspect the O-ring for damage and replace if necessary.

• | Clean and lubricate the fastener with Saturn Transaxle Fluid. Wipe off excess fluid.

1. Install the OSS.

Tighten
Tighten the output speed sensor (OSS) to 26 N·m (19 lb ft).

2. Connect the OSS harness connector. Push in the connector until a click is heard and pull back to confirm a positive engagement.
3. Lower the vehicle.
4. Check the transaxle fluid level.