For 1990-2009 cars

### Removal Procedure

1. Remove the fog lamp assembly. Refer to Front Fog Lamp Replacement in Lighting Systems.
2. Disconnect the electrical harness from the fog lamp.
3. Unscrew the headlamp adjuster from the capsule.
4. Remove the pushpin fasteners attaching the fog lamp capsule to the fog lamp capsule bracket.
5. Remove the fog lamp capsule.

### Installation Procedure

1. Position the fog lamp capsule into the fog lamp capsule bracket.
2. Screw the headlamp adjuster into the capsule.
3. Install the pushpin fasteners attaching the fog lamp capsule to the fog lamp capsule bracket.
4. Connect the electrical harness to the fog lamp capsule.
5. Aim the fog lamp. Refer to "Fog Lamp Aiming" in Lighting Systems.