For 1990-2009 cars

### Removal Procedure

1. Remove the headliner. Refer to Headlining Trim Panel Replacement in Interior Trim.
2. Remove the screws and the lower sunroof switch/console assembly.
3. Disconnect the harness from the motor.
4. Remove the screws and remove the sunroof motor.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

Notice: Do not pull the motor in with the attaching screws as this may result in damage to the drive cables.

Important: If the motor has been turned, or if the sunroof glass position has changed, the motor must be re-timed to the sunroof module. Refer to Sunroof Motor Synchronization .

1. Install the sunroof motor and connect it to the harness using the screws.

Tighten
Tighten the sunroof motor-to-sunroof module to 3-4 N·m (27-35 lb in).

2. Install the sunroof/console assembly with the screws.
3. Install the headliner. Refer to Headlining Trim Panel Replacement in Interior Trim.