For 1990-2009 cars

Replacement parts identified below by name, part number, or specification can be obtained from your dealer.

Part | Saturn Part Number
--- | ---
Air Cleaner Element (L24 or LL0 Engine) | 21000938
Surge Tank Pressure Cap | 10296465
Battery: The battery shield is designed for the size of the battery supplied with the vehicle. Always replace the battery with the same size. Battery life will be reduced if the battery shield is not used.
Automatic Transaxle Filter | 21003298
Engine Oil Filter | 21000872
PCV Valve | 25147308
Fuel Filter | 2100834
Windshield Wiper Blade Inserts (All Models) - Driver's Side - 21.5 inches (54.6 cm) - Passenger's Side - 20.0 inches (50.8 cm) | 21059149
Rear Wiper Blade Inserts (SW2) | 21035868
Spark Plugs: |
- SOHC (L24) Engine | NGK BKR4EA-11 (Saturn Part No. 21024922) (Gap at 1.0 mm [0.040 in.])
- DOHC (LL0) Engine | NGK BKR5EA-11 (Saturn Part No. 21024923) (Gap at 1.0 mm [0.040 in.])
DO NOT remove spark plugs from a hot engine. It may cause cylinder head thread damage.
The spark plugs available at your Saturn Retailer have the proper coatings of DAG and Vydex for your Saturn engine. These coatings prevent cylinder head, spark plug hole thread damage and keep the plug wires from sticking to the spark plugs.

Drive Belts: Automatically controlled by a tensioner.

### Tire Loading Information

| OCCUPANTS | VEHICLE CAPACITY WEIGHT
--- | --- | ---
MODEL | FRT | CTR | RR | TOTAL | LBS | KG
SEDAN (SL, SL1, SL2) | 2 | 0 | 3 | 5 | 864 | 392
COUPE (SC1, SC2) | 2 | 0 | 2 | 4 | 714 | 324
Wagon (SW2) | 2 | 0 | 3 | 5 | 864 | 392

MAXIMUM LOADING AT GVWR: SAME AS VEHICLE CAPACITY WEIGHT

### Tire Specification Information

MODEL |  | TIRE SIZE | SPEED RATING** | COLD TIRE PRESSURE PSI/KPA
--- | --- | --- | --- | ---
SEDAN (SL, SL1) | FRT | P185/65 R14 | S | 30/210
COUPE (SC1) | RR | 26/180
SEDAN (SL2) | FRT | P185/65 R15 | T | 30/210
COUPE (SC1)* | RR
Wagon (SW2) | 26/180
COUPE (SC2) | FRT | P195/60 R15 | H | 30/210
RR | 26/180
ALL | SPARE | T115/70 R14 | M | 60/415
If tires are hot, add 4 PSI (28 kPa) * SC1 Optional Tire ** Refer to the "Tire Warranty" section of the Owner's Handbook for an explanation of speed rating and for other important information about your tires.