For 1990-2009 cars

Application | Specifications
--- | ---
Metric | English
Battery Hold Down Retainer Nut and Screw | 9 N·m | 9 lb in
Battery Terminal Bolts | 17 N·m | 13 lb ft
Battery Tray-to-Rail | 7 N·m | 62 lb in
Fascia Support-to-Bumper Impact Bar | 3.5 N·m | 31 lb in
Fender-to-Front Body Hinge Pillar Bolt | 10 N·m | 89 lb in
Fender-to-Upper Motor Compartment Side Rail (Front) | 10 N·m | 89 lb in
Fog Lamp Bracket-to-Impact Bar Fasteners | 30 N·m | 22 lb ft
Head Hinge-to-Body Bolts | 25 N·m | 19 lb ft
Headlamp Housing Bolts (Coupe) | 7 N·m | 61 lb in
Headlamp Housing Fasteners | 6 N·m | 53 lb in
Hinge-to-Hood Bolts | 25 N·m | 19 lb ft
Hood Latch | 10 N·m | 89 lb in