For 1990-2009 cars

## Fog Lamps SC2 Models Only

For the type of bulb required for replacement, see Replacement Bulbs .

1. Turn off the fog lamp switch and allow bulbs to cool before changing.
2. Reach through the opening in the fascia to the rear of the fog lamp.
3. Rotate the bulb socket counterclockwise and remove it.
4. Remove the wire connector from the bulb by lifting the lock tab and pulling it away from the plastic base.
5. Remove the bulb and replace it with the appropriate bulb.

## Fog Lamps SL2, SW2 Models Only

For the type of bulb required for replacement, see Replacement Bulbs .

1. Turn off the fog lamp switch and allow bulbs to cool before changing.
2. Reach up from underneath the body panel, rotate the fog lamp bulb socket counterclockwise and remove it.
3. Rotate the fog lamp bulb from the harness.
4. Remove with the appropriate bulb.