For 1990-2009 cars

### Removal Procedure

1. While holding the dome lamp assembly, slide the lamp assembly towards the right side of vehicle to disengage the left side retainer.
2. Slide the dome towards the left to disengage to right side retainers.
3. Disconnect the wire harness and remove dome lamp.

### Installation Procedure

1. Connect the dome lamp wire harness to the dome lamp.
2. Slide the 2 right side retainers into place. Push the dome lamp to the right and upward to disengage remaining retainer.