For 1990-2009 cars

Table 1: | Data Link Connector-DLC
Table 2: | Park/Neutral Position Switch
Table 3: | Park/Neutral Position Switch
Table 4: | Park/Neutral Position Switch
Table 5: | Transaxle Actuators
Table 6: | Transaxle Fluid Temperature Sensor
Table 7: | Turbine Shaft Speed Sensor

#### Data Link Connector-DLC

Connector Part Information |

• | 12110250

• | Black

Cavity | Wire Color | Circuit Number | Wire Size | Circuit Function
--- | --- | --- | --- | ---
1 | PPL | 1807C | .35 | CLASS 2 TO SDM-1999 ONLY
2 | PPL | 1807A | .35 | CLASS2 TO PCM
3 | -- | -- | -- | --
4 | BLK | 350AG-AUTO 350BG-MAN | .35 | GROUND
5 | BLK | 452K | .35 | FLASH RTN FROM PCM
6 | DK BLU | 1446 | .35 | FLASH POWER AT PCM
7 | -- | -- | -- | --
8 | BLK/WHT | 1455B | .35 | PROGRAMMING MODE TO RKE MODULE
9 | TAN | 800 | .35 | SERIAL DATA TO SDM--1998 ONLY
10 | -- | -- | -- | --
11 | -- | -- | -- | --
12 | -- | -- | -- | --
13 | -- | -- | -- | --
14 | -- | -- | -- | --
15 | -- | -- | -- | --
16 | ORN | 340L | .35 | B+
Location: I/P Lower Left

#### Park/Neutral Position Switch

Connector Part Information |

• | 12059642

• | LT Gray

Cavity | Wire Color | Circuit Number | Wire Size | Circuit Function
--- | --- | --- | --- | ---
A | PPL | 6A | 3.0 | B+
B | PPL | 6X | 3.0 | FEED TO STARTER SOLENOID
Location: Engine Compartment-Lower Left

#### Park/Neutral Position Switch

Connector Part Information |

• | 12162260

• | Black

Cavity | Wire Color | Circuit Number | Wire Size | Circuit Function
--- | --- | --- | --- | ---
A | BLK/WHT | 771 | .50 | SHIFT SEL 1
B | YEL | 772 | .50 | SHIFT SEL 2
C | GRA | 773 | .50 | SHIFT SEL 3
D | WHT | 776 | .50 | SHIFT SEL D
E | LT GRN | 24C | .50 | REVERSE SWITCH
F | PNK | 239A | .50 | REVERSE SWITCH
Location: Engine Compartment-On Automatic Transaxle

#### Park/Neutral Position Switch

Connector Part Information |

• | 12089640

• | Black

Cavity | Wire Color | Circuit Number | Wire Size | Circuit Function
--- | --- | --- | --- | ---
A | BLK/WHT | 451K | 2.0 | GROUND
Location:Engine Compartment-On Automatic Transaxle

#### Transaxle Actuators

Connector Part Information |

• | 12092172

• | Black

Cavity | Wire Color | Circuit Number | Wire Size | Circuit Function
--- | --- | --- | --- | ---
A | LT GRN | 1527 | .50 | G3 POWER
B | YEL/BLK | 1223 | .50 | G3 ACTUATOR
C | LT GRN/BLK | 1527A | .50 | G4 POPWER
D | PPL | 898 | .50 | G4 ACTUATOR
E | WHT/BLK | 1526A | .50 | TCC ACTUATOR
F | DK BLU | 1530 | .50 | MLP ACTUATOR
G | RED | 1525 | .50 | MLP ACTUATOR
H | LT GRN | 1222 | .50 | G2 ACTUATOR
J | WHT | 1526 | .50 | G2/TCC POWER
K | TAN/BLK | 422 | .50 | TR PRESS SW
Location: Engine Compartment-Top of Automatic Transaxle

#### Transaxle Fluid Temperature Sensor

Connector Part Information |

• | 12092512

• | Black

Cavity | Wire Color | Circuit Number | Wire Size | Circuit Function
--- | --- | --- | --- | ---
A | BLK | 452T | .35 | FLUID TEMP RTN
B | ORN/BLK | 586 | .30 | FLUID TEMP SIGNAL
Location:Engine Compartment-Front Left

#### Turbine Shaft Speed Sensor

Connector Part Information |

• | 12052644

• | Gray

Cavity | Wire Color | Circuit Number | Wire Size | Circuit Function
--- | --- | --- | --- | ---
A | RED/BLK | 1230 | .35 | TURBINE SHAFT SPEED SIGNAL
B | DK BLU/WHT | 1231 | .35 | TURBINE SHAFT SPEED RTN
Location: Engine Compartment-On Transaxle Near Diff.