For 1990-2009 cars

### Removal Procedure

1. Depress center pins inward to release radio/HVAC controller cover push pin fasteners.

Important: Do not push center pins through fasteners.

2. Remove fasteners and pull radio/HVAC controller cover rearward.
3. Disconnect traction control/fog lamp/rear defog electrical connector, if equipped.
4. Rotate center deflectors down.
5. Place a small flat blade screwdriver between deflectors and pry slightly apart to disengage pivot point.
6. Remove deflectors.
7. Use a small flat blade screwdriver to disengage lock tabs on both sides of center outlet housing while pulling housing rearward.
8. Remove housing.

### Installation Procedure

1. Install center outlet hosing into opening in I/P retainer. Push in until tabs are flush with sides of housing.

Important: Small pivot pins are in center of housing. Large pivot pins are on sides of housing.

2. Rotate center outlets down and snap into housing.
3. Connect traction control/fog lamp/rear defog electrical connector, if equipped.
4. Install radio/HVAC control cover. Push in at clip locations.
5. Install push pins and lock.