For 1990-2009 cars

#### Tools Required

J-44228-A Axle Shaft Deflector Ring Installer

### Removal Procedure

Notice: The axle shaft deflector ring is designed to aid the transaxle seal from dirt and water intrusion. Deflector rings are installed on left and intermediate axle shafts, and rotate around the third lip of the transaxle seals. Improperly installed deflector rings may cause premature failure of transaxle seals, deflector rings, and axle shafts. Special tools J44280-1 and J44280-2 are required to properly install the deflector rings.

Important: If an axle shaft deflector ring is removed, a new deflector ring must be installed. Do not re-use axle shaft deflector rings that have been previously installed. If an axle shaft deflector ring is damaged, it should be replaced. Do not attempt to repair damaged deflector rings.

1. Remove the axle assemblies from vehicle. Refer to Wheel Drive Shaft Replacement .

Notice: Do not damage the smooth portion of the axle shaft assembly. The transaxle seal rides upon the smooth portion. If damaged, a leak can occur.

2. Clamp the axle shaft assembly in a vice. Use soft metal or wood between vice jaws to protect the shaft.
3. Remove the axle shaft deflector ring by prying the axle shaft deflector ring off with a screwdriver, or gently tap the axle shaft deflector ring off with a soft mallet.
4. Discard the axle shaft deflector ring. A new axle shaft deflector ring will be required for installation.

### Installation Procedure

1. Inspect the axle shaft assembly for any damage, repair as necessary.
2. Thoroughly clean the area that the deflector ring is to be installed upon.

Important: Ensure to notice which direction the deflector ring is installed. The cupped end of the deflector ring should face towards the transaxle seal.

3. Slide the deflector ring onto the drive axle shaft assembly by hand.

Important: The deflector ring must be fully seated against the tri-pot housing. If not fully seated, the deflector ring may cause premature failure to the transaxle seal.

4. Use special tool J-44228-A to install the axle deflector ring the remainder of the way. The deflector ring should bottom out against the tri-pot housing.
5. Install the drive axle assembly into the vehicle. Refer to Wheel Drive Shaft Replacement .