For 1990-2009 cars

### Removal Procedure

1. Hold the dome lamp assembly stable with hand.

Important: Be certain the screwdriver blade is placed between the dome lamp lens and the housing. Exerting pressure on the headliner may damage it and will not aid in removal of the lens.

2. Insert a small flat blade screwdriver into the slot.
3. Exert pressure to assembly, then twist the screwdriver to unsnap the lens from the retaining tab on the housing.

### Installation Procedure

1. Place the lens to dome lamp assembly.
2. Press the lens into place with light pressure.