For 1990-2009 cars

## Electronic Traction Control Switch Replacement Right Hand Drive Domestic Only

### Removal Procedure

1. Release the switch assembly lock tab with a small flat-blade screwdriver.
2. Disconnect the wire harness and remove the switch assembly.

### Installation Procedure

1. Connect the wire harness.
2. Insert the switch assembly, right side first, and snap into the instrument panel.

## Electronic Traction Control Switch Replacement Left Hand Drive Domestic Only

### Removal Procedure

1. Release the switch assembly lock tab with a small flat-blade screwdriver.
2. Disconnect the wire harness and remove the switch assembly.

### Installation Procedure

1. Connect the wire harness.
2. Insert the switch assembly, right side first, and snap into the instrument panel.