For 1990-2009 cars

### Removal Procedure

1. Remove the front fascia. Refer to Fascia Grille Replacement in Bumpers.
2. Remove the fasteners from fascia support brackets and energy absorber.
3. Remove the grille.

### Installation Procedure

1. Position the grille onto the vehicle.
2. Install the fasteners into the fascia support brackets and the energy absorber.
3. Install the front fascia. Refer to Fascia Grille Replacement in Bumpers.