For 1990-2009 cars

### Removal Procedure

1. Using a soft marker, mark around the striker for installation purposes.
2. Remove the screws, remove the striker and striker shim if present.

### Installation Procedure

1. Loosely install the striker and striker shim, if present, with screws.
2. Align the striker with marks made prior to removal.
3. Tighten the screws.
4. Check the door closing and align the striker as required.

Notice: Refer to Fastener Notice in the Preface section.

5. Tighten the striker screws.

Tighten
Tighten the door striker front bolts to 25 N·m (18 lb in).