For 1990-2009 cars

#### Tools Required

SA91107NE Wheel Stud Remover

Important: It may be necessary to cut off a portion of the stud with a die grinder to provide clearance to remove the stud due to interference with the steering knuckle. With stud loose in hub, rotate hub to position where least amount of interference between stud and knuckle exists.

1. UsingSA91107NE (or equivalent), remove wheel stud.
2. Start new wheel stud into hub.
3. Place four washers over stud.
4. Install wheel mounting nut with flat side toward washer.
5. Using a box-end wrench, tighten nut until stud is seated.