For 1990-2009 cars

Table 1: | Engine Oil
Table 2: | Engine Coolant
Table 3: | Hydraulic Brake System
Table 4: | Hydraulic Clutch System
Table 5: | Automatic/Manual Transaxle
Table 6: | Park Brake Cable Guides
Table 7: | Power Steering System
Table 8: | Key Lock Cylinders
Table 9: | Hood Latch Assembly
Table 10: | Hood and Door Hinges, Headlamp Door Assemblies, Rear Folding Seat, Trunk Lid Hinges
Table 11: | Door Hold-Open Check Links
Table 12: | Sunroof Track
Table 13: | Weatherstrips

#### Engine Oil

1.9L MFI (LLO) DOHC (VIN 7) | SAE 5W-30 or SAE 10W-30 Energy conserving oils designed with Starburst symbol.
1.9L MFI (L24) SOHC (VIN 8)

#### Engine Coolant

All Engines | 50/50 mixture of water (preferably distilled) and DEX-COOL® coolant conforming to Saturn P/N 21031164

#### Hydraulic Brake System

All Models | Delco Supreme 11 Brake Fluid or DOT 3 Brake Fluid (Saturn P/N 21013073)

#### Hydraulic Clutch System

Manual Transaxle | Delco Supreme 11 Brake Fluid or DOT 3 Brake Fluid (Saturn P/N 21013073)

#### Automatic/Manual Transaxle

Automatic and Manual Applications | Saturn Transaxle Fluid (Refer to "Saturn Parts Catalog" for correct part number).

#### Park Brake Cable Guides

All Models | Chassis lubricant (GM P/N 12377985 or equivalent) or lubricant meeting requirements of NLGI Grade 2, category LB or GC-LB.

#### Power Steering System

All Models with Power Steering | Saturn P/N 21007583 or GM Power Steering Fluid, GM P/N 1052884 (16 oz.) or 01050017 (32 oz.) or an equivalent fluid meeting GM specification 9985010.

#### Key Lock Cylinders

All Models | Lubricate with light oil or a graphite lubricant. (Do not use aerosols.)

#### Hood Latch Assembly

Pivots and Spring Anchor | Lubricate with SAE 5w-30 engine oil. (Do not use aerosols.)
Release Pawl | Lubricate with chassis grease meeting requirements of NLGI Grade 2, Category LB (GM P/N 1052497) or equivalent.

#### Hood and Door Hinges, Headlamp Door Assemblies, Rear Folding Seat, Trunk Lid Hinges

All Models | Lubricate with SAE 5w-30 engine oil. (Do not use aerosols.)

#### Door Hold-Open Check Links

All Models | Lubricate with Lubriplate® grease (aerosol) into the case; top, bottom, and sides. Use Lupriplate® 70 or equivalent to lubricate (Saturn P/N 21038869).

#### Sunroof Track

All Models | Use Lubriplate® (Saturn P/N 21038869) or equivalent to lubricate.

#### Weatherstrips

All Models | Lubricate with Dielectric Silicaon Grease (GM P/N12345579) or equivalent.