For 1990-2009 cars

### Right Front ESB Does Not Hold Motor

The expansion spring brakes (ESB)are used on both front and rear actuator motor assemblies. The spring expands to provide friction to prevent the modulator piston from being back-driven by hydraulic pressure. If the ESB allows the motor to be back-driven by hydraulic pressure. If the ESB allows the motor to be back-driven, the antilock telltale lamp will be turned On.

### Code Parameters

Code 41 sets if:

Right Front ESB does not hold motor.

This code can only set during initialization 13 km/h (8 mph).

This code can be set after an ABS stop if this channel did not get into ABS.

### Diagnostic Aids

The ESB is an internal component of the ABS motor pack and can not be serviced separately. If is is determined to be faulty, the motor pack must be replaced.

Use Scan tool to perform ABS motor tension release special test before removing motor pack.

When the ignition is cycled On, the ABS module verifies motors are in home position.

The ABS system will initialize (run motors down then up) when the vehicle is driven at least 13 km/h (8 mph) after start-up.

When attempting to diagnose an intermittent problem, use the Scan tool to review supplemental diagnostic information. The supplemental data can be used to duplicate a problem.

Select Malf History from Scan tool ABS menu.